21 0 -4.52 0 6.03 0 15.04 1 30.05 1 10.06 0 8.07 0 25.08 1 350.09 1 750.01 0 16.52 0 -4.03 0 85.04 0 90.05 1 10.06 0 8.07 0 50.08 1 150.09 0 0.010 0.0 800 15-1 -16.3 44.2 0.000 .002-2 -16.3 44.2 0.000 .002-3 -16.3 44.2 0.000 .002 1 7.8 -9.0 1.735 .002 1 -10.7 84.6 -0.441 .002 1 0.8 13.8 0.067 .002 2 7.8 -9.0 3.663 .003 2 -10.7 84.6 1.921 .003 2 0.8 13.8 -2.060 .003 3 7.8 -9.0 -3.002 .007 7

9.5 -6.1 -3.002 .007 47.0 105.0 x location y location strike dipdepth width length strike slip dip slip

(1st fault)

(2nd fault)

# of faults this parameter is fixed free to varysimplex version 4.0 input file format

(G. Lyzenga 1/15/99)

# of data points in data set

(data set) uncertainty value eastnorth verticalminus denotes reference sitestarting

"temperature"max # of iterations obsolete parameter (not used) location east location north observation types:

1displacement east2displacement north3displacement up4strain eee5strain een6strain enn7

line-of-sight displacement

SAR L.O.S

SAR elev. and azimuth

(type 7 only)